**BAND:PRS:1** The pump **shall** provide both a bolus and basal feature. **[BAND:URS:1]**

**BAND:PRS:2** The pump **shall** limit boluses to not exceed 25 units. **[BAND:RISK:10]**

dfssdfsdfdsfsd